{"text_format":"3","workbook":"xlsx","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":8,"n_cols":7,"rows_kept":8,"merged":[[0,0,0,6],[6,0,6,4]]}
["温州市中西医结合医院空调清洗工程量报价清单"]
["序号","项目名称","单位","数量","服务操作质量说明","单价","小计"]
[1,"风机盘管机清洗消毒","台",550,"1、断电、拆取进出风口外壳过滤网清洗消毒；\n2、进风空间、涡轮（排污），叶轮、电机清洗消毒；\n3、出风风管积尘清洁清洗消毒；\n4、蒸发器铝翅片清洗消毒；\n5、积水盘清洗、排水通畅；\n6、部件安装、清理开机运行。"]
[2,"天花机清洗消毒","台",20,"1、断电、拆取外壳过滤网清洗消毒；\n2、拆取风轮清洗消毒；\n3、蒸发器铝翅片清洗消毒；\n4、积水盘清洗、排水通畅；\n5、部件安装、清理开机运行。"]
[3,"风管机清洗","台",0,"1、断电、拆取进出风口外壳过滤网清洗消毒；\n2、进风空间、涡轮清洗消毒；\n3、出风风管积尘清洁清洗消毒；"]
[4,"变风量空调系统清洗","台",40,"1、主机检查，关闭电源；\n2、拆开风口及过滤器清洗消毒；\n3、表冷面清洗消毒、托盘清洁排污水路畅通；\n4、主机舱清理，出风口清洗消毒；\n5、部件安装、清理开机运行。"]
["注：清洗设备数量为暂定，最终结算以实际清洗数量计入。",{"$nulls":4},"合计"]
[{"$nulls":4},"                             投标人（盖单位章）："]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0}